{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":7,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZA-D"]
[]
[]
[]
[]
["","","","","FUA100AVEB9 / FUA100AVEB9 / RZA200D7Y1B","FUA71AVEB9 / FUA71AVEB9 / FUA71AVEB9 / RZA200D7Y1B","FUA125AVEB9 / FUA125AVEB9 / RZA250D7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","19.0 (1)","19.0 (1)","22.0 (1)"]
["Hlađenje prostora","SEER","","","7.01","7.39","6.10"]
["","ηs,c","","%","278","292","241"]
["","Godišnja potrošnja električne energije","","kWh/a","1,625","1,543","2,163"]
["","Kapacitet","Pdesign","kW","19.0","19.0","22.0"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","11.2","11.2","12.1"]
["","SCOP/A","","","4.10","4.15","4.10"]
["","Godišnja potrošnja električne energije","","kWh/a","3,825","3,779","4,132"]
["","ηs,h","","%","161","163","161"]
["Kapacitet grejanja","Nom.","","kW","22.4 (2)","22.4 (2)","24.0 (2)"]
["Beleške","","","","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]