{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":9,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FUA100AVEB / RZAG71M7Y1B","FUA71AVEB / RZAG71M7Y1B","FUA71AVEB / FUA71AVEB / RZAG100M7Y1B","FUA100AVEB / RZAG100M7Y1B","FUA125AVEB / RZAG125M7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","12.1 (1)"]
["Space cooling","SEER","","","6.89","7.02","8.82","6.42","6.39"]
["","Godišnja potrošnja električne energije","","kWh/a","345","339","377","518","1,136"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.50","9.50","12.1"]
["","Klasa energetske efikasnosti","","","A++","A++","A+++","A++"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","4.70","4.70","7.80","7.80","9.52"]
["","SCOP/A","","","4.28","4.20","4.73","4.50","4.26"]
["","Klasa energetske efikasnosti","","","A+","A+","A++","A+"]
["","Godišnja potrošnja električne energije","","kWh/a","1,537","1,567","2,309","2,427","3,129"]
["Kapacitet grejanja","Nom.","","kW","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","13.5 (2)"]
["Beleške","","","","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Hlađenje: T2: unutrašnja temp. 26,6°CDB, 19,4 °CWB, spoljna temp. 48°CDB [Btu/hr/W]","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]