{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":16,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FUA71AVEB / FUA71AVEB / RZQG100L8Y1B","FUA71AVEB / FUA71AVEB / RZQG125L8Y1B","FUA100AVEB / RZQG100L8Y1B","FUA125AVEB / RZQG125L8Y1B","FUA100AVEB9 / RZQG100L8Y1B","FUA125AVEB9 / RZQG125L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG100L8Y1B","FUA71AVEB9 / FUA71AVEB9 / RZQG125L8Y1B","FUA100AVEB9 / RZQG71L8Y1B","FUA71AVEB / RZQG71L8Y1B","FUA71AVEB9 / RZQG71L8Y1B","FUA100AVEB / RZQG71L8Y1B"]
["Kapacitet hlađenja","Nom.","","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["Hlađenje prostora","SEER","","","","","","","","","","","6.42","6.42","6.42","6.42"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","371","371","371","371"]
["","Kapacitet","Pdesign","kW","","","","","","","","","6.80","6.80","6.80","6.80"]
["","Klasa energetske efikasnosti","","","","","","","","","","","A++","A++","A++","A++"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","","","","","","","","","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","","","","","","","","","4.20","4.20","4.20","4.20"]
["","Klasa energetske efikasnosti","","","","","","","","","","","A+","A+","A+","A+"]
["","Godišnja potrošnja električne energije","","kWh/god.","","","","","","","","","2,534","2,534","2,534","2,534"]
["Nominalna efikasnost","Godišnja potrošnja električne energije","","kWh","","","","","","","","","","835","835"]
["","EER","","","","","","","","","","","4.07","4.07","4.07","4.07"]
["","COP","","","","","","","","","","","","4.08","4.08"]
["","Direktiva o energetskom označavanju","Hlađenje","","","","","","","","","","","A","A"]
["","","Grejanje","","","","","","","","","","","A","A"]
["Kapacitet grejanja","Nom.","","kW","","","","","","","","","","7.50","7.50"]
["Beleške","","","","","","","","","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nominalni rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","","","","","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Beleške","","","","","","","","","","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","","","","","","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]