{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":82,"n_cols":11,"rows_kept":82,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FUA-A"]
[]
[]
[]
[]
["","","","","","FUA71AVEB9","FUA100AVEB9","FUA125AVEB9","FUA71AVEB (Archived)","FUA100AVEB (Archived)","FUA125AVEB (Archived)"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","","","","41","46","47"]
["","","","Srednji","dBA","","","","38","42","43"]
["","","","Nizak","dBA","","","","35","39","40"]
["","Hlađenje","","Medium","dBA","","","","38","42","43"]
["","","","Nizak","dBA","","","","35","39","40"]
["","","","Visok","dBA","","","","41","46","47"]
["Standardni pribor","Priručnik za upotrebu","","","","","","","1","1","1"]
["","Priručnik za instalaciju","","","","","","","1","1","1"]
["","Ispusno crevo","","","","","","","1","1","1"]
["","Termoizolaciona cev","","","","","","","3","3","3"]
["","Kablovske obujmice","","","","","","","10","10","10"]
["","Traka za crevo","","","","","","","1","1","1"]
["","Zaptivno sredstvo","","","","","","","4","4","4"]
["","Podloška pričvrsne ploče","","","","","","","1","1","1"]
["","odvodna spojnica","","","","","","","1","1","1"]
["","Netkani tekstil","","","","","","","1","1","1"]
["","Podloška","","","","","","","8","8","8"]
["","Pričvrsni zavrtanj za ispusno crevo","","","","","","","5","5","5"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Kapacitet hlađenja","Ukupan kapacitet","","Nom.","kW","","","","","","12.1"]
["Cevne spojnice","Tečnost","","SP","mm","","","","9.52","9.52","9.52"]
["","Gas","","SP","mm","","","","15.9","15.9","15.9"]
["","Ispusni otvor","","","","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Sound power level","Hlađenje","","","dBA","","","","59","64","65"]
["","Grejanje","","","dBA","","","","59","64"]
["Dimenzije","Uređaj","","Širina","mm","","","","950","950","950"]
["","","","Dubina","mm","","","","950","950","950"]
["","","","Visina","mm","","","","198","198","198"]
["Kućište","Materijal","","","","","","","Smola","Smola","Smola"]
["","Boja","","","","","","","Sveža bela","Sveža bela","Sveža bela"]
["Težina","Uređaj","","","kg","","","","25.0","26.0","26"]
["Ventilator","Brzina protoka vazduha","Grejanje","Visok","m³/min","","","","23.0","31.0","32.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Nizak","m³/min","","","","16.0","20.0","20.5"]
["","","Hlađenje","Nizak","m³/min","","","","16.0","20.0","20.5"]
["","","","Medium","m³/min","","","","19.5","25.5","26.5"]
["","","","Visok","m³/min","","","","23.0","31.0","32.5"]
["Ispusna visina","mm","","","","","","","600","600","600"]
["Kapacitet grejanja","Ukupan kapacitet","","Nom.","kW","","","","","","13.5"]
["Kućište","Boja","","","","Sveža bela","Sveža bela","Sveža bela"]
["","Materijal","","","","Smola","Smola","Smola"]
["Dimenzije","Uređaj","","Visina","mm","198","198","198"]
["","","","Širina","mm","950","950","950"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","950","950","950"]
["Težina","Uređaj","","","kg","25.0","26.0","26.0"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","23.0","31.0","32.5"]
["","","","Srednji","m³/min","19.5","25.5","26.5"]
["","","","Nizak","m³/min","16.0","20.0","20.5"]
["","","Grejanje","Visok","m³/min","23.0","31.0","32.5"]
["","","","Srednji","m³/min","19.5","25.5","26.5"]
["","","","Nizak","m³/min","16.0","20.0","20.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","59","64","65"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","41","46","47"]
["","","","Srednji","dBA","38","42","43"]
["","","","Nizak","dBA","35","39","40"]
["","Grejanje","","Visok","dBA","41","46","47"]
["","","","Srednji","dBA","38","42","43"]
["","","","Nizak","dBA","35","39","40"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","9.52","9.52"]
["","Gas","","SP","mm","15.9","15.9","15.9"]
["","Ispusni otvor","","","","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)","VP25 (OD Ø32.0)"]
["Ispusna visina","mm","","","","600","600","600"]
["Standardni pribor","Installation manual","","","","1","1","1"]
["","Thermal insulation tube","","","","3","3","3"]
["","Non woven fabric","","","","1","1","1"]
["","Drain joint","","","","1","1","1"]
["","Hose band","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Drain hose","","","","1","1","1"]
["","Fixing screw for drain hose","","","","5","5","5"]
["","Sealing material","","","","4","4","4"]
["","Tie-wraps","","","","10","10","10"]
["","Washer","","","","8","8","8"]
["","Washer fixing plate","","","","1","1","1"]
["Kapacitet hlađenja","Ukupan kapacitet","","Nom.","kW","","","12.10"]
["Kapacitet grejanja","Ukupan kapacitet","","Nom.","kW","","","13.5"]