{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVA-A"]
[]
[]
[]
[]
["","","","","","FVA71AMVEB","FVA100AMVEB","FVA125AMVEB","FVA140AMVEB"]
["Kapacitet hlađenja","Ukupan kapacitet","","Nom.","kW","","","12.10","13.40"]
["Kapacitet grejanja","Ukupan kapacitet","","Nom.","kW","","","13.5","15.5"]
["Kućište","Boja","","","","Sveža bela","Sveža bela","Sveža bela","Sveža bela"]
["Dimenzije","Uređaj","","Visina","mm","1850","1850","1850","1850"]
["","","","Širina","mm","600","600","600","600"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","270","350","350","350"]
["Težina","Uređaj","","","kg","42","50","50","50"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","18","28","28","30"]
["","","","Srednji","m³/min","16","25","26","28"]
["","","","Nizak","m³/min","14","22","24","26"]
["","","Grejanje","Visok","m³/min","18","28","28","30"]
["","","","Srednji","m³/min","16","25","26","28"]
["","","","Nizak","m³/min","14","22","24","26"]
["Nivo zvučne snage","Hlađenje","","","dBA","55","62","63","65"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","43","50","51","53"]
["","","","Srednji","dBA","41","47","48","51"]
["","","","Nizak","dBA","38","44","46","48"]
["","Grejanje","","Visok","dBA","43","50","51","53"]
["","","","Srednji","dBA","38","44","46","48"]
["","","","Nom.","dBA","41","47","48","51"]
["Povezivanje cevi","Tečnost","","SP","mm","9.52","9.52","9.52","9.52"]
["","Gas","","SP","mm","15.9","15.9","15.9","15.9"]
["","Ispusni otvor","","","","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26","I.D. 20/O.D. 26"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","Hole protection rubber","","","","2","2","2","2"]
["","Cover","","","","1","1","1","1"]
["","Dew proof material","","","","1","1","1","1"]
["","Remote control wiring","","","","1","1","1","1"]
["","Bracket for installation","","","","1","1","1","1"]
["","Operation manual","","","","1","1","1","1"]
["","Bush","","","","1","1","1","1"]
["","Installation pattern","","","","1","1","1","1"]
["","Insulation for fitting for gas pipe","","","","1","1","1","1"]
["","Insulation for fitting for liquid pipe","","","","1","1","1","1"]
["","Screws","","","","5","5","5","5"]
["","Tie-wraps","","","","5","5","5","5"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50/60","50/60","50/60","50/60"]
["","Napon","","","V","220-240/220","220-240/220","220-240/220","220-240/220"]