{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":11,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FVQ100CVEB / RZQG71L8Y1B","FVQ71CVEB / RZQG71L8Y1B","FVQ140CVEB / RZQG100L8Y1B","FVQ100CVEB / RZQG100L8Y1B","FVQ125CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG125L8Y1B","FVQ140CVEB / RZQG140L7Y1B"]
["Kapacitet hlađenja","Nom.","","kW","","6.8","","9.5","12.0","","13.4"]
["Hlađenje prostora","SEER","","","6.31","6.23","5.61","5.61","5.61","5.61"]
["","Godišnja potrošnja električne energije","","kWh/a","378","383","593","593","748.663","749"]
["","Kapacitet","Pdesign","kW","6.80","6.80","9.50","9.5","12.00","12.00"]
["","Klasa energetske efikasnosti","","","A++","A++","A+","A+","A+","A+"]
["Grejanje prostora (Prosečna klima)","Kapacitet","Pdesign","kW","6.33","6.33","11.30","11.3","11.30","11.30"]
["","SCOP/A","","","4.05","4.05","4.20","4.2","3.87","3.87"]
["","Klasa energetske efikasnosti","","","A+","A+","A+","A+","A","A"]
["","Godišnja potrošnja električne energije","","kWh/a","2,189","2,189","3,767","3,767","4,087.855","4,088"]
["Nominalna efikasnost","Annual energy consumption","","kWh","","1,010","","1,245","1,870","","2,085"]
["","EER","","","","3.37","","3.81","3.21","","3.21"]
["","COP","","","","3.64","","4.14","3.70","","3.61"]
["","Direktiva o energetskom označavanju","Hlađenje","","","A","","A","A"]
["","","Grejanje","","","A","","A","A"]
["Kapacitet grejanja","Nom.","","kW","","7.5","","10.8","13.5","","15.5"]
["Beleške","","","","","(1) - Godišnja potročnja energije je u skladu sa direktivom o energetskom označavanju 2002/31/EC","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU","","(1) - EER/COP u skladu sa programom Eurovent 2012, za upotrebu isključivo van EU"]
["","","","","","(2) - SEER i SCOP su u skladu sa EN 14825","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)","","(2) - Nominalna efikasnost: hlađenje na 35°/27° nominalnog opterećenja, grejanje na 7°/20° nominalnog opterećenja)"]