{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":7,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-A9 / RXM-A9"]
[]
[]
[]
[]
["","","","","FVXM25A3V1B9 / RXM25A5V1B9","FVXM35A3V1B9 / RXM35A5V1B9","FVXM50A3V1B9 / RXM50A5V1B9"]
["Kapacitet hlađenja","Min.","","kW","1.3","1.4","1.4"]
["","Nom.","","kW","2.4","3.4","5"]
["","Maks.","","kW","3.5","4","5.8"]
["Kapacitet grejanja","Min.","","kW","1.3","1.4","1.4"]
["","Nom.","","kW","3.4","4.5","5.8"]
["","Maks.","","kW","4.7","5.8","8.1"]
["Nominalna efikasnost","EER","","","4.47","4.01","3.81"]
["","COP","","","4.55","3.9","3.81"]
["","Godišnja potrošnja električne energije","","kWh","268","424","656"]
["","Direktiva o energetskom označavanju","Hlađenje","","A","A","A"]
["","","Grejanje","","A","A","A"]
["Hlađenje prostora","Klasa energetske efikasnosti","","","A+++","A++","A++"]
["","Kapacitet","Pdesign","kW","2.4","3.4","5"]
["","SEER","","","8.55","8.11","7.3"]
["","Godišnja potrošnja električne energije","","kWh/god.","98","147","240"]
["Grejanje prostora (Prosečna klima)","Klasa energetske efikasnosti","","","A++","A++","A+"]
["","Kapacitet","Pdesign","kW","2.3","2.8","4.1"]
["","SCOP/A","","","4.65","4.63","4.31"]
["","Pdh Kapacitet grejanja na -10°C","","kW","2.03","2.34","3.58"]
["","Godišnja potrošnja električne energije","","kWh/god.","693","847","1330"]
["Opseg energetske efikasnosti","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Beleške","","","","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m.","(1) - Nom. rashladni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 27°CDB, 19°CWB, spoljna temperatura: 35°CDB, odgovarajuća dužina cevi rashladnog fluida: 5 m, visinska razlika: 0 m."]
["","","","","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m.","(2) - Nominalni grejni kapaciteti se zasnivaju na sledećem: unutrašnja temperatura: 20 °CDB, spoljna temperatura: 7°CDB, 6°CWB,odgovarajuće cevi za rashladnu tečnost: 5m, visinska razlika: 0m."]
["","","","","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada","(3) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(4) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]