{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":8,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXM-B"]
[]
[]
[]
[]
["","","","","","FVXM25B2V1B","FVXM35B2V1B","FVXM50B2V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.02","0.02","0.03"]
["","Grejanje","","Nom.","kW","0.02","0.03","0.03"]
["Kućište","Boja","","","","Bela","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","600","600","600"]
["","","","Širina","mm","750","750","750"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","238","238","238"]
["Težina","Uređaj","","","kg","17","17","17"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","8.7","9.2","11.6"]
["","","","Srednji","m³/min","7","7","9"]
["","","","Nizak","m³/min","4.9","4.9","6.6"]
["","","","Nečujan rad","m³/min","4.1","4.1","5.4"]
["","","Grejanje","Visok","m³/min","9.2","9.8","12.8"]
["","","","Srednji","m³/min","7.2","7.2","10"]
["","","","Nizak","m³/min","5.6","5.6","8.4"]
["","","","Nečujan rad","m³/min","4.1","4.1","5.9"]
["Nivo zvučne snage","Hlađenje","","","dBA","52","53","61"]
["","Grejanje","","","dBA","52","53","62"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","38","39","44"]
["","","","Srednji","dBA","32","32","38"]
["","","","Nizak","dBA","25","25","31"]
["","","","Nečujan rad","dBA","20","20","27"]
["","Grejanje","","Visok","dBA","38","39","46"]
["","","","Srednji","dBA","32","32","40"]
["","","","Nizak","dBA","25","25","35"]
["","","","Nečujan rad","dBA","19","19","29"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","675","675","675"]
["Povezivanje cevi","Tečnost","","SP","mm","6.4","6.4","6.4"]
["","Gas","","SP","mm","9.5","9.5","12.7"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC466A90","ARC466A90","ARC466A90"]
["","Žičani daljinski upravljač","","","","BRC073A1","BRC073A1","BRC073A1"]
["Standardni pribor","FVXM25B2V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Wireless remote control","","","","1","1","1"]
["","AAA dry-cell batteries","","","","2","2","2"]
["","General safety precautions","","","","1","1","1"]
["","Operation manual","","","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2","2"]
["","Remote control holder","","","","1","1","1"]
["","Screw bag","","","","1","1","1"]
["Napajanje","Ime","","","","V1","V1","V1"]
["","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["Standardni pribor","FVXM35B2V1B","","","","","1"]
["","FVXM50B2V1B","","","","","","1"]