{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":52,"n_cols":6,"rows_kept":52,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FVXTM-B"]
[]
[]
[]
[]
["","","","","","FVXTM30B2V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.02"]
["","Grejanje","","Nom.","kW","0.03"]
["Kućište","Boja","","","","Bela"]
["Dimenzije","Uređaj","","Visina","mm","600"]
["","","","Širina","mm","750"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","238"]
["Težina","Uređaj","","","kg","17"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","9"]
["","","","Srednji","m³/min","6.7"]
["","","","Nizak","m³/min","4.8"]
["","","","Nečujan rad","m³/min","4"]
["","","Grejanje","Visok","m³/min","9.4"]
["","","","Srednji","m³/min","6.8"]
["","","","Nizak","m³/min","5.3"]
["","","","Nečujan rad","m³/min","4"]
["Nivo zvučne snage","Hlađenje","","","dBA","53"]
["","Grejanje","","","dBA","53"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","20"]
["","Grejanje","","Visok","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","19"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","675"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35"]
["","Gas","","SP","mm","9.5"]
["","Ispusni otvor","","","","VP20 (I.D. 20/O.D. 26)"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC466A90"]
["","Žičani daljinski upravljač","","","","BRC073A1"]
["Standardni pribor","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","2"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Ime","","","","V1"]
["","Faza","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]
["Beleške","","","","","(1) - Hlađenje: unutrašnja temp. 27°CDB, 19°CWB; spoljna temp. 35°CDB, 24°CWB; odgovarajuća dužina cevi: 5m"]
["","","","","","(2) - Grejanje: unutrašnja temp. 20°CDB; spoljna temp. 7°CDB, 6°CWB; odgovarajuće cevi za rashladnu tečnost: 5m"]
["","","","","","(3) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]