{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":6,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","MCK70YV"]
[]
[]
[]
[]
["","","","","","MCK70YVM"]
["Tip","","","","","Prečistač i ovlaživač vazduha"]
["Primena","","","","","Podni tip"]
["Kućište","Boja","","","","Bela (N9. 0)"]
["Dimenzije","Uređaj","","Visina","mm","600 (5)"]
["","","","Širina","mm","395"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","287"]
["Težina","Uređaj","","","kg","12.5"]
["Primenljiva površina prostorije","m²","","","","48 (1), 96 (2)"]
["CADR","m³/h","","","","375"]
["Prečišćavanje vazduha","Ulazna snaga","","Turbo","kW","0.066"]
["","","","M","kW","0.016"]
["","","","L","kW","0.01"]
["","","","Nečujan","kW","0.008"]
["Vlaženje vazduha","Ulazna snaga","","Turbo","kW","0.068"]
["","","","M","kW","0.018"]
["","","","L","kW","0.012"]
["","","","Nečujan","kW","0.011"]
["","Kapacitet rezervoara vode","","","l","3.6"]
["Nivo zvučnog pritiska","Prečišćavanje vazduha","","Turbo","dBA","54"]
["","","","Srednji","dBA","37"]
["","","","Nizak","dBA","27"]
["","","","Nečujan","dBA","18"]
["","Vlaženje vazduha","","Turbo","dBA","54"]
["","","","Srednji","dBA","37"]
["","","","Nizak","dBA","27"]
["","","","Nečujan","dBA","23"]
["Ventilator","Brzina protoka vazduha","Prečišćavanje vazduha","Turbo","m³/h","420"]
["","","","Srednji","m³/h","210"]
["","","","Nizak","m³/h","132"]
["","","","Nečujan","m³/h","60"]
["","","Vlaženje vazduha","Turbo","m³/h","420"]
["","","","Srednji","m³/h","210"]
["","","","Nizak","m³/h","132"]
["","","","Nečujan","m³/h","102"]
["Način sakupljanja prašine","","","","","Elektrostatički HEPA filter"]
["Način dezodorisanja","","","","","Fleš strimer + dezodorišuci katalizator"]
["Standardni pribor","Operation manual","","","","1"]
["","Electrostatic HEPA filter","","","","1"]
["","Deodorising filter","","","","1"]
["","Caster","","","","4"]
["","Humidifying filter","","","","1"]
["Električni kabl","m","","","","2"]
["Napajanje","Faza","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50/60"]
["","Napon","","","V","220-240/220-230"]
["Beleške","","","","","(1) - Površina prostorije odgovara radu jedinice uz maksimalnu brzinu ventilatora (HH). Površina prostorije označava prostor u kojem određena količina čestica prašine može da bude uklonjena za 30 minuta."]
["","","","","","(2) - Preračunato sa testiranih vrednosti u NRCC standarde u skladu sa JEM1467 test metodom."]
["","","","","","(3) - Nivoi radnog zvuka predstavljaju prosek vrednosti izmerenih na 1 m udaljenosti od prednje, leve, desne i gornje ploče uređaja. (Oni odgovaraju vrednostima merenja u gluvoj komori)"]