{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":39,"n_cols":20,"rows_kept":39,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RX-K"]
[]
[]
[]
[]
["","","","","","RX20K2V1B","RX20K5V1B","RX20K5V1B9","RX25K2V1B","RX25K5V1B","RX25K5V1B9","RX35K2V1B","RX35K5V1B","RX35K5V1B9","RX50KV1B","RX50K2V1B","RX60KV1B","RX60K2V1B","RX71KV1B","RX71K2V1B"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","","","","","","","","","","51.3"]
["","","Grejanje","Super nisko","m³/min","","","","","","","","","","51.3"]
["","","","Super nisko","cfm","","","","","","","","","","1812"]
["","","Grejanje","Super nisko","cfm","","","","","","","","","","1812"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550","550","550","550","550","550","550","735","734","735","734","735","734"]
["","","","Širina","mm","658","658","658","658","658","658","658","658","658","870","870","870","870","870","870"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","275","275","275","275","275","275","275","275","275","320","373","320","373","320","373"]
["Težina","Uređaj","","","kg","28","28","28","28","28","28","28","28","28","44","46.0","49","49.0","49","49.0"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10 (1)","-10","","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46","46","46","46","46","","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15","-15","-15","-15","-15","-15","-15","-15","","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18","18","18","18","18","","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","46","46","46","46","46","46","48","48","48","47","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","47","","49","","52"]
["","Grejanje","","Visok","dBA","47","47","47","47","47","47","48","48","48","48","","49","","52"]
["","","","Nom.","dBA","","","","","","","","","","","48","","49","","52"]
["Rashladni fluid","Tip","","","","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A","R-410A"]
["","Količina","","","kg","0.74","0.74","0.74","0.74","0.74","0.74","1.0","1.0","1.0","1.13","1.13","1.45","1.45","1.45","1.45"]
["","Količina","","","tCO2Eq","1.5","1.5","1.5","1.5","1.5","1.5","2.1","2.1","2.1","2.4","2.36","3.0","3.03","3.0","3.03"]
["","GWP (potencijal globalnog otopljavanja)","","","","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","15","15","15","15","15","15","15","15","15","30","30.0","30","30.0","30","30.0"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","12","12","12","12","12","12","12","12","12","20","20.0","20","20.0","20","20.0"]
["Standardni pribor","Installation manual","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["","Drain plug (only heat pump models)","","","","1","1","1","1","1","1","1","1","1","1","1","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50","50","50","50","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB","(1) - Radni opseg u kombinaciji sa FTX-J3: min. 10°CDB ~ maks. 46°CDB"]
["Standardni pribor","Drain cap","","","","","","","","","","","","","9","9","9","9","9","9"]