{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":11,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-B"]
[]
[]
[]
[]
["","","","","","RXC20BV1B","RXC25BV1B","RXC35BV1B","RXC50BV1B","RXC60BV1B","RXC71BV1B"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","","","","","54"]
["Rashladno sredstvo","Charge","","","TCO2Eq","","","","","","0.776"]
["","GWP (potencijal globalnog otopljavanja)","","","","","","","","","675"]
["","Količina","","","kg","","","","","","1.15"]
["","Tip","","","","","","","","","R-32"]
["Piping connections","Razlika nivoa","IU - OU","Maks.","m","","","","","","20.0"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","","","","","0,017 (za dužinu cevi preko 7,5 m)"]
["Kompresor","Type","","","","","","","","","Hermetički klatni"]
["Dimenzije","Uređaj","","Širina","mm","","","","","","930"]
["","","","Dubina","mm","","","","","","350"]
["","","","Visina","mm","","","","","","695"]
["Težina","Uređaj","","","kg","","","","","","45"]
["Power supply","Phase","","","","","","","","","1~"]
["","Frekvencija","","","Hz","","","","","","50"]
["","Napon","","","V","","","","","","220-240"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550","615","615"]
["","","","Širina","mm","658","658","658","845","845"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","273","273","273","300","300"]
["Težina","Uređaj","","","kg","24","24","26","39","39"]
["Kompresor","Tip","","","","Hermetički klatni","Hermetički klatni","Hermetički klatni","Hermetički klatni","Hermetički klatni"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","10","10","10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","45","45","46","51","54"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","0.55","0.55","0.75","1","1.1"]
["","Količina","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675","675","675"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20","20","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15.0","15.0","15.0","20.0","20.0"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240"]