{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXC-C"]
[]
[]
[]
[]
["","","","","","RXC20CV1B","RXC25CV1B","RXC35CV1B","RXC50CV1B","RXC60CV1B","RXC71CV1B"]
["Dimenzije","Uređaj","","Visina","mm","550","550","550","615","615","695"]
["","","","Širina","mm","658","658","658","845","845","930"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","273","273","273","300","300","350"]
["Težina","Uređaj","","","kg","24","24","26","39","39","45"]
["Kompresor","Tip","","","","Hermetički klatni","Hermetički klatni","Hermetički klatni","Hermetički klatni","Hermetički klatni","Hermetički klatni"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","10","10","10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","45","45","46","51","54","54"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","0.55","0.55","0.75","1","1.1","1.15"]
["","Količina","","","tCO2Eq","0.371","0.371","0.506","0.675","0.743","0.776"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0","675.0","675.0","675.0"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20","20","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)","0,017 (za dužinu cevi preko 7,5 m)"]
["","Razlika nivoa","IU - OU","Maks.","m","15.0","15.0","15.0","20.0","20.0","20.0"]
["Napajanje","Faza","","","","1~","1~","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240","220-240","220-240"]