{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":7,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXLG-M"]
[]
[]
[]
[]
["","","","","","RXLG25M2V1B","RXLG35M2V1B"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Super nisko","m³/min","30.6","30.6"]
["","","Grejanje","Super nisko","m³/min","27.2","27.2"]
["","","","Super nisko","cfm","1080","1080"]
["","","Grejanje","Super nisko","cfm","960","960"]
["Dimenzije","Uređaj","","Visina","mm","550","550"]
["","","","Širina","mm","858","858"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","330","330"]
["Težina","Uređaj","","","kg","40","40"]
["Kompresor","Type","","","","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10"]
["","","","Maks.","°CDB","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-25","-25"]
["","","","Maks.","°CWB","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","48","48"]
["","","","Nizak","dBA","44","44"]
["","Grejanje","","Visok","dBA","49","49"]
["","","","Nizak","dBA","45","45"]
["Rashladni fluid","Tip","","","","R-410A","R-410A"]
["","Količina","","","kg","1","1"]
["","Količina","","","tCO2Eq","2.1","2.1"]
["","GWP (potencijal globalnog otopljavanja)","","","","2087.5","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","20","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - IU","Maks.","m","15","15"]
["Standardni pribor","Installation manual","","","","1","1"]
["","Drain plug","","","","1","1"]
["Napajanje","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor"]