{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":9,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXM-N"]
[]
[]
[]
[]
["","","","","","RXM42N2V1B","RXM50N2V1B","RXM60N2V1B","RXM71N2V1B"]
["Dimenzije","Uređaj","","Visina","mm","734","734","734","734"]
["","","","Širina","mm","870","870","870","870"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","373","373","373","320"]
["Težina","Uređaj","","","kg","50","50","50","56"]
["Kompresor","Type","","","","Hermetički zatvoren klatni kompresor","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-10","-10","-10","-10"]
["","","","Maks.","°CDB","46","46","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-15","-15","-15","-15"]
["","","","Maks.","°CWB","18","18","18","18"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48.0","48.0","48.0","47"]
["","Grejanje","","Nom.","dBA","48.0","49.0","49.0","48"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32","R-32"]
["","Količina","","","kg","1.10","1.15","1.15","1.15"]
["","Količina","","","tCO2Eq","0.75","0.78","0.78","0.78"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675","675.0"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","30","30","30","30.0"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","20","20","20","20.0"]
["Standardni pribor","Installation manual","","","","1","1","1","1"]
["","Refrigerant charge label","","","","1","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1","1"]
["","Drain cap","","","","3","3","3","3"]
["","Drain plug","","","","1","1","1","1"]
["Napajanje","Faza","","","","1~","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240","220-240"]
["Kompresor","Tip","","","","","Hermetički zatvoren klatni kompresor"]