{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":59,"n_cols":12,"rows_kept":59,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RXS-K"]
[]
[]
[]
[]
["","","","","","RXS20K3V1B","RXS20K2V1B","RXS25K3V1B","RXS25K2V1B","RXS35K2V1B","RXS42K2V1B","RXS50K2V1B"]
["Nivo zvučnog pritiska","Grejanje","","Visok","dBA","47","","47","","48","48","48"]
["","Hlađenje","","Visok","dBA","46","","46","","48","48","48"]
["Standardni pribor","čep ispusnog otvora","","","","","","","","1","1","1"]
["","Priručnik za instalaciju","","","","1","","1","","1","1","1"]
["Rashladno sredstvo","Charge","","","TCO2Eq","2.1","","2.1","","2.5","2.7","3.5"]
["","GWP (potencijal globalnog otopljavanja)","","","","2,087.5","","2,087.5","","2,087.5","2,087.5","2,087.5"]
["","Punjenje","","","kg","1.0","","1.0","","1.2","1.3","1.7"]
["","Tip","","","","R-410A","","R-410A","","R-410A","R-410A","R-410A"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","780","","780","","780","790","670"]
["","","Grejanje","Superniska","o/min","740","","740","","740","780","670"]
["Cevne spojnice","Razlika nivoa","IU - OU","Maks.","m","15","","15","","15","15","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 10m)","","0,02 (za dužinu cevovoda preko 10m)","","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)","0,02 (za dužinu cevovoda preko 10m)"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","","Hermetički zatvoren klatni kompresor","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Dimenzije","Uređaj","","Širina","mm","765","","765","","765","765","825"]
["","","","Dubina","mm","285","","285","","285","285","300"]
["","","","Visina","mm","550","","550","","550","550","735"]
["Težina","Uređaj","","","kg","34","","34","","34","39","47"]
["Ventilator","Brzina protoka vazduha","Grejanje","Super nisko","cfm","","","","","904","960","1,522"]
["","","Hlađenje","Super nisko","cfm","","","","","1,063","1,080","1,727"]
["Power supply","Faza","","","","1~","","1~","","1~","1~","1~"]
["","Frekvencija","","","Hz","50","","50","","50","50","50"]
["","Napon","","","V","220-240","","220-240","","220-240","220-240","220-240"]
["Beleške","","","","","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V","(1) - 220V"]
["","","","","","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V","(2) - 230V"]
["","","","","","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V","(3) - 240V"]
["","","","","","(4) - SL: Nečujan nivo rada ventilatora za trenutni protok vazduha","","(4) - SL: Nečujan nivo rada ventilatora za trenutni protok vazduha","","(4) - Sadrži fluorisane gasove sa efektom staklene bašte","(4) - Sadrži fluorisane gasove sa efektom staklene bašte","(4) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Standardni pribor","Spojnica (odvod)","","","","1","","1"]
["Beleške","","","","","(5) - Sadrži fluorisane gasove sa efektom staklene bašte","","(5) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Dimenzije","Uređaj","","Visina","mm","","550","","550"]
["","","","Širina","mm","","765","","765"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","285","","285"]
["Težina","Uređaj","","","kg","","34","","34"]
["Motor ventilatora","Brzina","Hlađenje","Superniska","o/min","","780","","780"]
["","","Grejanje","Superniska","o/min","","740","","740"]
["Kompresor","Tip","","","","","Hermetički zatvoren klatni kompresor","","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","-10","","-10"]
["","","","Maks.","°CDB","","46","","46"]
["","Grejanje","Spolja","Min.","°CWB","","-15","","-15"]
["","","","Maks.","°CWB","","18","","18"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","","46","","46"]
["","Grejanje","","Visok","dBA","","47","","47"]
["Rashladni fluid","Tip","","","","","R-410A","","R-410A"]
["","Količina","","","kg","","1.0","","1.0"]
["","Količina","","","tCO2Eq","","2.1","","2.1"]
["","GWP (potencijal globalnog otopljavanja)","","","","","2087.5","","2087.5"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","20","","20"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","","0,02 (za dužinu cevovoda preko 10m)","","0,02 (za dužinu cevovoda preko 10m)"]
["","Razlika nivoa","IU - OU","Maks.","m","","15","","15"]
["Standardni pribor","Installation manual","","","","","1","","1"]
["","Joint (drain)","","","","","1","","1"]
["Napajanje","Faza","","","","","1~","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","","50","","50"]
["","Napon","","","V","","220-240","","220-240"]