{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZA-D"]
[]
[]
[]
[]
["","","","","","RZA200D7Y1B","RZA250D7Y1B"]
["Dimenzije","Uređaj","","Visina","mm","870","870"]
["","","","Širina","mm","1,100","1,100"]
["","","","Dubina","mm","460","460"]
["Težina","Uređaj","","","kg","117","117"]
["Kompresor","Type","","","","Hermetički zatvoren pužni kompresor","Hermetički zatvoren pužni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-20","-20"]
["","","","Maks.","°CDB","46","46"]
["","Grejanje","Spolja","Min.","°CWB","-20","-20"]
["","","","Maks.","°CWB","15","15"]
["Nivo zvučne snage","Hlađenje","","","dBA","73","76"]
["","Grejanje","","","dBA","76 (1)","79 (1)"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","53","57"]
["","Grejanje","","Nom.","dBA","60","63"]
["Rashladno sredstvo","Tip","","","","R-32","R-32"]
["","Količina","","","kg","5","5"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675"]
["Piping connections","Tečnost","","SP","mm","9.52","9.52"]
["","Gas","","SP","mm","22.2","22.2"]
["","Dužina cevovoda","Maks.","OU - IU","m","100","100"]
["","","Sistem","Bez punjenja","m","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju"]
["Standardni pribor","Priručnik za instalaciju","","","","1","1"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","1","1"]
["","Kablovske obujmice","","","","2","2"]
["","Samolepljiva etiketa  fluor (F-gas)","","","","1","1"]
["","Spojne cevi","","","","6","6"]
["Power supply","Phase","","","","3~","3~"]
["","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","380-415","380-415"]
["Struja - 50Hz","Maksimalna amperaža osigurača (MFA)","","","A","20","20"]
["Beleške","","","","","(1) - U skladu sa ENER Lot 21","(1) - U skladu sa ENER Lot 21"]