{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-A"]
[]
[]
[]
[]
["","","","","","RZAG35A2V1B","RZAG50A2V1B","RZAG60A2V1B"]
["Dimenzije","Uređaj","","Visina","mm","734","734","734"]
["","","","Širina","mm","870","870","870"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","373","373","373"]
["Težina","Uređaj","","","kg","52","52","52"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Nivo zvučne snage","Hlađenje","","","dBA","62.0","63.0","64.0"]
["","Grejanje","","","dBA","62.0","63.0","64.0"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48.0","49.0","50.0"]
["","Grejanje","","Nom.","dBA","48.0","49.0","50.0"]
["Rashladni fluid","Tip","","","","","R-32"]
["","Količina","","","kg","1.55","1.55","1.55"]
["","GWP (potencijal globalnog otopljavanja)","","","","675.0","675.0","675.0"]
["","Količina","","","tCO2Eq","1.05","1.05","1.05"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.50","12.7","12.7"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","50","50","50"]
["","","Sistem","Bez punjenja","m","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)","0,02 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","30.0","30.0","30.0"]
["Standardni pribor","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","1","1","1"]
["","LOT10 Energy Label","","","","1","1","1"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Napajanje","Faza","","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","","220-240"]