{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":45,"n_cols":8,"rows_kept":45,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZAG-B"]
[]
[]
[]
[]
["","","","","","RZAG35B5V1B","RZAG50B5V1B","RZAG60B5V1B"]
["Dimenzije","Uređaj","","Visina","mm","734","734","734"]
["","","","Širina","mm","870","870","870"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","373","373","373"]
["Težina","Uređaj","","","kg","52","52","52"]
["Kompresor","Tip","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-20","-20","-20"]
["","","","Maks.","°CDB","52","52","52"]
["","Grejanje","Spolja","Min.","°CWB","-21","-21","-21"]
["","","","Maks.","°CWB","18","18","18"]
["Nivo zvučne snage","Hlađenje","","","dBA","62","63","64"]
["","Grejanje","","","dBA","62","63","64"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48","49","50"]
["","Grejanje","","Nom.","dBA","48","49","50"]
["Rashladni fluid","Tip","","","","R-32","R-32","R-32"]
["","Količina","","","kg","1.55","1.55","1.55"]
["","GWP (potencijal globalnog otopljavanja)","","","","675","675","675"]
["","Količina","","","tCO2Eq","1.05","1.05","1.05"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35","6.35"]
["","Gas","","SP","mm","9.52","12.7","12.7"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","50","50","50"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","002 (za dužinu cevovoda preko 30m)","002 (za dužinu cevovoda preko 30m)","002 (za dužinu cevovoda preko 30m)"]
["","Razlika nivoa","IU - OU","Maks.","m","30","30","30"]
["Standardni pribor","RZAG35B5V1B","","","","1"]
["","Installation manual","","","","1","1","1"]
["","Refrigerant charge label","","","","1","1","1"]
["","Multilingual fluorinated greenhouse gases labels","","","","1","1","1"]
["","General safety precautions","","","","General safety precautions","General safety precautions","General safety precautions"]
["","LOT10 Energy Label","","","","LOT10 Energy Label","LOT10 Energy Label","LOT10 Energy Label"]
["","Drain cap","","","","3","3","3"]
["","Drain plug","","","","1","1","1"]
["Opseg energetske efikasnosti","","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Napajanje","Faza","","","","1~","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50","50"]
["","Napon","","","V","220-240","220-240","220-240"]
["Beleške","","","","","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada","(1) - Pogledajte zasebne crteže za podatke o opsegu rada"]
["","","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte","(3) - Sadrži fluorisane gasove sa efektom staklene bašte"]
["Standardni pribor","RZAG50B5V1B","","","","","1"]
["","RZAG60B5V1B","","","","","","1"]