{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":54,"n_cols":7,"rows_kept":54,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQ-C"]
[]
[]
[]
[]
["","","","","","RZQ200C7Y1B","RZQ250C7Y1B"]
["Dimenzije","Uređaj","","Visina","mm","1,680"]
["","","","Širina","mm","930"]
["","","","Dubina","mm","765"]
["Težina","Uređaj","","","kg","183.0"]
["Kompresor","Type","","","","Hermetički zatvoren pužni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-5.0"]
["","","","Maks.","°CDB","46.0"]
["","Grejanje","Spolja","Min.","°CWB","-15.0"]
["","","","Maks.","°CWB","15.0"]
["Nivo zvučne snage","Hlađenje","","","dBA","78.0"]
["","Grejanje","","","dBA","78.0"]
["Rashladno sredstvo","Tip","","","","R-410A"]
["","Količina","","","kg","8.3"]
["","GWP (potencijal globalnog otopljavanja)","","","","2,087.5"]
["Piping connections","Tečnost","","SP","mm","9.52"]
["","Gas","","SP","mm","22.2"]
["","Dužina cevovoda","Maks.","OU - IU","m","100"]
["","","Sistem","Bez punjenja","m","30"]
["Standardni pribor","Priručnik za instalaciju","","","","1"]
["","Spojne cevi","","","","4"]
["Power supply","Phase","","","","3N~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","380-415"]
["Struja - 50Hz","Maksimalna amperaža osigurača (MFA)","","","A","25"]
["Beleške","","","","","(1) - Izvor napajanja FDQ unutrašnje jedinice je odvojen"]
["","","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["Dimenzije","Uređaj","","Visina","mm","","1680"]
["","","","Širina","mm","","930"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","","765"]
["Težina","Uređaj","","","kg","","184.0"]
["Kompresor","Tip","","","","","Hermetički zatvoren pužni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","","-5.0"]
["","","","Maks.","°CDB","","46.0"]
["","Grejanje","Spolja","Min.","°CWB","","-15.0"]
["","","","Maks.","°CWB","","15.0"]
["Nivo zvučne snage","Hlađenje","","","dBA","","78.0"]
["","Grejanje","","","dBA","","78.0"]
["Rashladni fluid","Količina","","","kg","","9.3"]
["","GWP (potencijal globalnog otopljavanja)","","","","","2087.5"]
["","Količina","","","tCO2Eq","","19.4"]
["Povezivanje cevi","Tečnost","","SP","mm","","12.70"]
["","Gas","","SP","mm","","22.2"]
["Cevne spojnice","Dužina cevovoda","Maks.","OU - IU","m","","100"]
["","","Sistem","Bez punjenja","m","","30"]
["Standardni pribor","Installation manual","","","","","1"]
["","Connection pipes","","","","","4"]
["Izvor napajanja","Frekvencija","","","Hz","","50"]
["Struja - 50Hz","Struja - 50Hz-=-Maksimalna amperaža osigurača (MFA)-=-A","","","A","","25"]