{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":9,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","","RZQG71L8Y1B","RZQG100L8Y1B (Archived)","RZQG125L8Y1B (Archived)","RZQG140L7Y1B (Archived)"]
["Dimenzije","Uređaj","","Visina","mm","990","1,430","1,430","1,430"]
["","","","Širina","mm","940","940","940","940"]
["","","","Dubina","mm","320","320","320","320"]
["Težina","Uređaj","","","kg","80.0","101.0","101.0","101.0"]
["Kompresor","Type","","","","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor","Hermetički zatvoren klatni kompresor"]
["Radni opseg","Hlađenje","Spolja","Min.","°CDB","-15.0","-15.0","-15.0","-15.0"]
["","","","Maks.","°CDB","50.0","50.0","50.0","50.0"]
["","Grejanje","Spolja","Min.","°CWB","-20.0","-20.0","-20.0","-20.0"]
["","","","Maks.","°CWB","15.5","15.5","15.5","15.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","64.0","66.0","67.0","69.0"]
["","Grejanje","","","dBA","64.0","66.0","67.0","69.0"]
["Nivo zvučnog pritiska","Hlađenje","","Nom.","dBA","48","50","51","52"]
["","Grejanje","","Nom.","dBA","50","52","53","53"]
["","Noćni tihi režim","","Novo 1","dBA","43","45","45","45"]
["Rashladno sredstvo","Tip","","","","R-410A","R-410A","R-410A","R-410A"]
["","Količina","","","kg","2.9","4.0","4.0","4.0"]
["","GWP (potencijal globalnog otopljavanja)","","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Piping connections","Tečnost","","SP","mm","9.52","9.52","9.52","9.52"]
["","Gas","","SP","mm","15.9","15.9","15.9","15.9"]
["","Dužina cevovoda","Maks.","OU - IU","m","50","75","75","75"]
["","","Sistem","Odgovarajuća","m","70","90","90","90"]
["","","","Bez punjenja","m","30","30","30","30"]
["","Dodatna punjenje rashladnog sredstva","","","kg/m","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju","Pogledati priručnik za instalaciju"]
["","Razlika nivoa","IU - OU","Maks.","m","30.0","30.0","30.0","30.0"]
["","","IU - IU","Maks.","m","0.5","0.5","0.5","0.5"]
["Standardni pribor","Kablovske obujmice","","","","2","2","2","2"]
["","Priručnik za instalaciju","","","","1","1","1","1"]
["Power supply","Phase","","","","3N~","3N~","3N~","3N~"]
["","Frekvencija","","","Hz","50","50","50","50"]
["","Napon","","","V","380-415","380-415","380-415","380-415"]
["Struja - 50Hz","Maksimalna amperaža osigurača (MFA)","","","A","16","25","25","25"]
["Beleške","","","","","(1) - 3 sa mogućnošću punjenja","(1) - 3 sa mogućnošću punjenja","(1) - 3 sa mogućnošću punjenja","(1) - 3 sa mogućnošću punjenja"]
["","","","","","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama","(2) - Pogledajte zasebne crteže za podatke o elektroinstalacijama"]
["","","","","","(3) - PED (Direktiva o opremi pod pritiskom): sklop = kategorija l: isključeno iz okvira PED zbog člana 1, stavke 3.6 dokumenta 97/23/EC","(3) - PED (Direktiva o opremi pod pritiskom): sklop = kategorija l: isključeno iz okvira PED zbog člana 1, stavke 3.6 dokumenta 97/23/EC","(3) - PED (Direktiva o opremi pod pritiskom): sklop = kategorija l: isključeno iz okvira PED zbog člana 1, stavke 3.6 dokumenta 97/23/EC","(3) - PED (Direktiva o opremi pod pritiskom): sklop = kategorija l: isključeno iz okvira PED zbog člana 1, stavke 3.6 dokumenta 97/23/EC"]
["","","","","","(4) - EN/IEC 61000-3-11: Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A","(4) - EN/IEC 61000-3-11: Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A","(4) - EN/IEC 61000-3-11: Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A","(4) - EN/IEC 61000-3-11: Evropski/internacionalni tehnički standard koji postavlja granice varijacija, fluktuacija i podrhtavanja napona u nisko-naponskim javnim mrežama, za opremu sa nominalnom strujom jačine ≤ 75A"]