{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-BS"]
[]
[]
[]
[]
["","","","","","CTXA15B2V1BS"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.02"]
["","Grejanje","","Nom.","kW","0.02"]
["Kućište","Boja","","","","Srebrna"]
["Dimenzije","Uređaj","","Visina","mm","295"]
["","","","Širina","mm","798"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","189"]
["Težina","Uređaj","","","kg","11.5"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","11"]
["","","","Srednji","m³/min","8.2"]
["","","","Nizak","m³/min","6.1"]
["","","","Nečujan rad","m³/min","4.6"]
["","","Grejanje","Visok","m³/min","10.9"]
["","","","Srednji","m³/min","8.7"]
["","","","Nizak","m³/min","6.4"]
["","","","Nečujan rad","m³/min","4.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","57"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","21"]
["","Grejanje","","Visok","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","21"]
["Rashladni fluid","GWP (potencijal globalnog otopljavanja)","","","","675"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35"]
["","Gas","","SP","mm","9.5"]
["","Ispusni otvor","","","","18"]
["Kontrolni sistemi","Infracrveni daljinski upravljač","","","","ARC466A58"]
["","Žičani daljinski upravljač","","","","BRC073"]
["Standardni pribor","Installation manual","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Air filter","","","","2"]
["","Infrared remote control","","","","1"]
["","Remote controller mounting plate","","","","1"]
["","Screw bag","","","","1"]
["Napajanje","Ime","","","","V1"]
["","Faza","","","","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]