{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":6,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXA-CB"]
[]
[]
[]
[]
["","","","","","CTXA15C2V1BB"]
["Apsorbovana snaga","Hlađenje","","Nom.","kW","0.020"]
["","Grejanje","","Nom.","kW","0.020"]
["Kućište","Colour","","","","Crna"]
["Dimenzije","Uređaj","","Visina","mm","295"]
["","","","Širina","mm","798"]
["","","","Dubina","mm","189"]
["Težina","Uređaj","","","kg","11.5"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","11.0"]
["","","","Medium","m³/min","8.2"]
["","","","Nizak","m³/min","6.1"]
["","","","Nečujan rad","m³/min","4.6"]
["","","Grejanje","Visok","m³/min","10.9"]
["","","","Medium","m³/min","8.7"]
["","","","Nizak","m³/min","6.4"]
["","","","Nečujan rad","m³/min","4.5"]
["Nivo zvučne snage","Hlađenje","","","dBA","57"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","39"]
["","","","Medium","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","21"]
["","Grejanje","","Visok","dBA","39"]
["","","","Srednji","dBA","32"]
["","","","Nizak","dBA","25"]
["","","","Nečujan rad","dBA","21"]
["Rashladno sredstvo","GWP (potencijal globalnog otopljavanja)","","","","675.0"]
["Piping connections","Tečnost","","SP","mm","6.35"]
["","Gas","","SP","mm","9.50"]
["","Ispusni otvor","","","","18"]
["Kontrolni sistemi","Infrared remote control","","","","ARC466A85"]
["","Žičani daljinski upravljač","","","","BRC073A1"]
["Standardni pribor","Priručnik za instalaciju","","","","1"]
["","Priručnik za upotrebu","","","","1"]
["","Filter za vazduh","","","","2"]
["","Infracrveni daljinski upravljač","","","","1"]
["","Noseća ploča daljinskog upravljača","","","","1"]
["","Vreća za zavrtnje","","","","1"]
["","Poklopac zavrtnja","","","","2"]
["","AAA suve baterije","","","","2"]
["","Opšta upozorenja u vezi sa bezbednošću","","","","1"]
["Power supply","Ime","","","","V1"]
["","Phase","","","","1~"]
["","Frekvencija","","","Hz","50"]
["","Napon","","","V","220-240"]