{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":49,"n_cols":7,"rows_kept":49,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","CTXM-R"]
[]
[]
[]
[]
["","","","","","CTXM15R2V1B","CTXM15R5V1B"]
["Ulazna snaga","Hlađenje","","Nom.","kW","0.029","0.029"]
["","Grejanje","","Nom.","kW","0.023","0.023"]
["Kućište","Boja","","","","Bela","Bela"]
["Dimenzije","Uređaj","","Visina","mm","295","295"]
["","","","Širina","mm","778","778"]
["","","","Dimenzije-=-Uređaj-=-Dubina-=-mm","mm","272","272"]
["Težina","Uređaj","","","kg","10","10"]
["Ventilator","Brzina protoka vazduha","Hlađenje","Visok","m³/min","10.5","10.5"]
["","","","Srednji","m³/min","7.5","7.5"]
["","","","Nizak","m³/min","5.7","5.7"]
["","","","Nečujan rad","m³/min","4.3","4.3"]
["","","Grejanje","Visok","m³/min","9.3","9.3"]
["","","","Srednji","m³/min","8.2","8.2"]
["","","","Nizak","m³/min","6.2","6.2"]
["","","","Nečujan rad","m³/min","5.1","5.1"]
["Nivo zvučne snage","Hlađenje","","","dBA","57","57"]
["","Grejanje","","","dBA","54","54"]
["Nivo zvučnog pritiska","Hlađenje","","Visok","dBA","41","41"]
["","","","Srednji","dBA","33","33"]
["","","","Nizak","dBA","25","25"]
["","","","Nečujan rad","dBA","19","19"]
["","Grejanje","","Visok","dBA","39","39"]
["","","","Srednji","dBA","34","34"]
["","","","Nizak","dBA","26","26"]
["","","","Nečujan rad","dBA","20","20"]
["Povezivanje cevi","Tečnost","","SP","mm","6.35","6.35"]
["","Gas","","SP","mm","9.5","9.5"]
["","Ispusni otvor","","","","18","18"]
["Control systems","Infracrveni daljinski upravljač","","","","ARC466A67","ARC466A67"]
["Kontrolni sistemi","Žičani daljinski upravljač","","","","BRC073A1","BRC073A1"]
["Standardni pribor","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","AAA dry-cell batteries","","","","2","2"]
["","WLAN adapter kit","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Napajanje","Ime","","","","V1","V1"]
["","Faza","","","","1~","1~"]
["Izvor napajanja","Frekvencija","","","Hz","50","50"]
["","Napon","","","V","220-240","220-240"]