{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Nivo zvučnog pritiska","Grejanje","Visok","dBA","47","47"]
["","","Nečujan rad","dBA","19","19"]
["","","Nizak","dBA","23","23"]
["","Hlađenje","Nečujan rad","dBA","21","21"]
["","","Nizak","dBA","33","33"]
["","","Visok","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Hlađenje","Nom.","dBA","39","39"]
["Standardni pribor","Priručnik za instalaciju","","","1","1"]
["","Priručnik za upotrebu","","","1","1"]
["","Infracrveni daljinski upravljač","","","1","1"]
["","Baterije","","","2","2"]
["","Držač daljinskog upravljača","","","1","1"]
["","Noseća ploča","","","1","1"]
["","Fotokatalitički filter za vazduh od titanijumapatita","","","2","2"]
["","Pričvrsni zavrtnji unutrašnje jedinice","","","2","2"]
["Kontrolni sistemi","Infrared remote control","","","ARC466A9","ARC466A9"]
["Povezivanje cevi","Tečnost","SP","mm","6.35","6.35"]
["","Gas","SP","mm","9.5","9.5"]
["","Ispusni otvor","","","18","18"]
["Ulazna snaga","Hlađenje","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Grejanje","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Nivo zvučne snage","Hlađenje","","dBA","59","59"]
["","Grejanje","","dBA","62","62"]
["Dimenzije","Uređaj","Širina","mm","900","900"]
["","","Dubina","mm","215","215"]
["","","Visina","mm","298","298"]
["Kućište","Boja","","","Bela","Bela"]
["Težina","Uređaj","","kg","12","12"]
["Power supply","Faza","","","1~","1~"]
["","Frekvencija","","Hz","50","50"]
["","Ime","","","V1","V1"]
["","Napon","","V","220-240","220-240"]
["Beleške","","","","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu.","(1) - Pri povezivanju sa višestrukom spoljnom jedinicom, pogledajte specifikacije za tu višestruku spoljnu jedinicu."]
["","","","","(2) - 220V","(2) - 220V"]
["","","","","(3) - 230V","(3) - 230V"]
["","","","","(4) - 240V","(4) - 240V"]