{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":3,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","RRDQ-V1"]
[]
[]
[]
[]
["","","RRDQ220V1"]
["Standardni pribor","Crevo za punjenje od 1/4 inča sa kuglastim ventilom (crveno) dužine 152 cm (AR344)","Crevo za punjenje od 1/4 inča sa kuglastim ventilom (crveno) dužine 152 cm (AR344)"]
["","Crevo za punjenje od 1/4 inča sa kuglastim ventilom (plavo) dužine 152 cm (AR345)","Crevo za punjenje od 1/4 inča sa kuglastim ventilom (plavo) dužine 152 cm (AR345)"]
["","Filter (TF011)","Filter (TF011)"]
["","Filter kaseta za susenje sa poroznim kuglicama","Filter kaseta za susenje sa poroznim kuglicama"]
["","Kontrolno staklo od 1/4 inča","Kontrolno staklo od 1/4 inča"]
["","Konusna spojnica od 1/4 inča, ženska sa obe strane","Konusna spojnica od 1/4 inča, ženska sa obe strane"]
["","Uputstvo za upotrebu RRDQ220V1 (IM0496)","Uputstvo za upotrebu RRDQ220V1 (IM0496)"]
["","Adapter za punjenje rashladnog fluida - upotrebljava se za recikliranje R134a (dodatna oprema)","Adapter za punjenje rashladnog fluida - upotrebljava se za recikliranje R134a (dodatna oprema)"]
["Beleške","","(1) - Specifikacije su podložne promenama bez prethodne najave"]
["","","(2) - Brzine recikliranja se razlikuju u zavisnosti od uslova"]
["","","(3) - Prilikom recikliranja R134a, pogledajte stranu 11 uputstva za upotrebu"]
["","","(4) - Rezultat recikliranja zavisi od stepena zagađenosti rashladnog fluida koji se recikira"]